**Meter Notifications classifications**

|  |  |  |  |
| --- | --- | --- | --- |
| Pending | Critical | Success | Warning |
| Token is not processed yet | High Energy Usage | Enter a token | Low units |
| Meter load Control is not processed yet | Low/Bad power factor | Turn the geyser of or on | High temperature |
| Heater load control is not processed yet | Current overload | Turn the meter on or off | Low temperature |
|  | High active power |  | Meter |
|  | Low active energy |  | Temper detection |
|  | Low active power |  |  |
|  | Low frequency |  |  |
|  | Meter reset |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |